|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IL1 | 10.2 | 2nd paragraph | te | During this low EMD time, the EMD level may exceed *V*E,PICC during one short period of 16/*fc* if it never  exceeds 4 times *V*E,PICC.  Comment: Only a single bigger noise event is allowed while we expect the receiver to be able to tolerate more than one if spaced far enough of each other. | Allow more than one large EMD event with a minimum inter-space of one ETU (?). |  |